**1 – General Rules and Practices**

|  |  |
| --- | --- |
| No. | General Rule or Practice |
| 1 | **https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png All instructions over serial: *are terminated with three bytes of*0xFF 0xFF 0xFF** ie: decimal: 255 or hex: 0xFF or ansichar: ÿ or binary: 11111111 ie byte ndt[3] = {255,255,255}; write(ndt,3); or print(“\xFF\xFF\xFF”); or print(“ÿÿÿ”) |
| 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png All instructions and parameters are in ASCII |
| 3 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png All instructions are in lowercase letters |
| 4 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Blocks of code and enclosed within braces { } can not be sent over serial this means if, for, and while commands can not be used over serial |
| 5 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png A space char 0x20 is used to separate command from parameters. |
| 6 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png There are no spaces in parameters unless specifically stated |
| 7 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Nextion uses integer math and does not have real or floating support. |
| 8 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Assignment are non-complex evaluating fully when reaching value after operator. |
| 9 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Comparison evaluation is non-complex, but can be joined (see && and ||). |
| 10 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Instructions over serial are processed on receiving termination (see [1.1](https://nextion.tech/resource/documents/instruction-set/#s1_1)) |
| 11 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Character escaping is performed using two text chars: \r creates 2 bytes 0x0D 0x0A, \” 0x22 and \\ for 0x5C |
| 12 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Nextion does not support order of operations. sys0=3+(8\*4) is invalid. |
| 13 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png 16-bit 565 Colors are in decimal from 0 to 65535 (see [5.Note](https://nextion.tech/resource/documents/instruction-set/#s5_note)) |
| 14 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Text values must be encapsulated with double quotes: ie “Hello” |
| 15 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sK.png Items which are specific to Enhanced Models are noted with https://cdn.nextion.tech/wp-content/uploads/2019/07/sK.png |
| 16 | Transparent Data Mode (used by https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png addt and https://cdn.nextion.tech/wp-content/uploads/2019/07/sKP.png wept commands)   1. MCU sending to Nextion    1. MCU sends command. ie: wept 30,20ÿÿÿ or addt 1,0,320ÿÿÿ    2. Nextion requires ~5ms to prepare for transparent mode data transfer    3. Nextion sends “Ready” 0xFE 0xFF 0xFF 0xFF Return Data (see [7.32](https://nextion.tech/resource/documents/instruction-set/#s7_FE))    4. MCU can now send specified quantity (20) of raw bytes to Nextion    5. Nextion receives raw bytes from MCU until specified quantity (20) is received    6. Nextion sends “Finished” 0xFD 0xFF 0xFF 0xFF Return Data (see [7.31](https://nextion.tech/resource/documents/instruction-set/#s7_FD))    7. MCU and Nextion can proceed to next command   Note: Nextion will remain waiting at step 5 until every byte of specified quantity is received. – During this time Nextion can not execute any other commands, and may indeed hang if the MCU fails to deliver the number of bytes as specified by the command parameter. – data quantity limited by serial buffer (all commands+terminations + data < 1024) |
| 17 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Only component attributes in green and non readonly system variables can be assigned new values at runtime. All others are readonly at runtime with the exception of .objname |
| 18 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Numeric values can now be entered with byte-aligned hex. ie: n0.val=0x01FF |
| 19 | **https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Advanced**. Address mode is an advanced technique prepending the serial instruction with two bytes for the address. Two byte address is to be sent in little endian order, ie: 2556 is sent 0xFC 0x09. By default, the Nextion address is 0 and does not require two byte prefixing. When the two byte addressing is used, Nextion will only respond to the command if its address matches the two byte prefix, or the transmitted address is 65535 broadcast. See the addr system variable. |
| 20 | **https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Advanced**. Protocol Reparse mode is an advanced technique that allows users to define their own incoming protocol and incoming serial data handling. When in active Protocol Reparse mode, incoming serial data will not be processed natively by the Nextion firmware but will wait in the serial buffer for processing. To exit active Protocol Reparse mode, recmod must be set back to passive (ie: in Nextion logic as recmod=0), which can not be achieved via serial. Send DRAKJHSUYDGBNCJHGJKSHBDNÿÿÿ via serial to exit active mode serially. Most HMI applications will not require Protocol Reparse mode and should be skipped if not fully understood. |
| 21 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Commenting user code inside Events uses the double-slash (two characters of forward slash / ) technique. See [2.30](https://nextion.tech/resource/documents/instruction-set/#s2_30) for proper usage. |
|  |  |

https://cdn.nextion.tech/wp-content/uploads/2019/07/sT.png : Basic https://cdn.nextion.tech/wp-content/uploads/2019/07/sK.png : Enhanced https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png : Intelligent https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png : All https://cdn.nextion.tech/wp-content/uploads/2019/07/sTK.png : Basic or Enhanced https://cdn.nextion.tech/wp-content/uploads/2019/07/sKP.png : Enhanced or Intelligent

**2 – Assignment Statements**

|  |  |  |  |
| --- | --- | --- | --- |
| No. | Data Type | Operator | Description/Example (see [1.8](https://nextion.tech/resource/documents/instruction-set/#s1_8) and [1.17](https://nextion.tech/resource/documents/instruction-set/#s1_17)) |
| 1 | Text | = | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Assignment. Right side will be evaluated with result placed in left side. Component .txt-maxl needs to be large enough to hold result. |
| t0.txt=”Hello” |
| 2 | Text | += | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Text Addition. Will concatenate left side with right side with result placed left side. ie t0.txt+=”Hello” is equivalent to t0.txt=t0.txt+”Hello”. t0.txt=”-“+t0.txt becomes t0.txt=t0.txt+”-“. Use temp variable to prepend. va0.txt=t0.txt t0.txt=”-“+va0.txt |
| t0.txt+=” World” // append ” World” to t0.txt //When contents of t0.txt is “Hello” becomes “Hello World” |
| 3 | Text | -= | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Text Subtraction. Will remove right side (a specified numeric amount of characters to remove) from end of left side and result placed in left side. |
| t0.txt-=4 or t0.txt=t0.txt-4 // remove last 4 chars from t0.txt |
| 4 | Text | \ | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Escape Character. (see [1.11](https://nextion.tech/resource/documents/instruction-set/#s1_11)) Supported is \r hex 0x0D 0x0A, \” hex 0x22, \\ hex 0x5C, |
| t0.txt=”\r” |
| 5 | Text | == | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Boolean Equality. Evaluate left side to right side. If both left and right sides are the same creates a true condition |
| if(t0.txt==va0.txt) |
| 6 | Text | != | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Boolean Inequality. Evaluate left side to right side. If both left and right sides are different creates a true condition |
| if(t0.txt!=va0.txt) |
| 7 | Numeric | = | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Assignment. Right side of equation will be evaluated and result placed in left side. If more than one operator on right side, full evaluation and assignment will occur at each operator. |
| n0.val=bauds // places bauds value in n0.val component |
| 8 | Numeric | += | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Numeric Addition. Adds value of left side and right side with result placed in left side. n0.val+=4 is equivalent to n0.val=n0.val+4 |
| n0.val+=va0.val |
| 9 | Numeric | -= | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Numeric Subtraction. Subtracts right side from left side with result placed in left side. n0.val-=4 is equivalent to n0.val=n0.val-4 |
| n0.val-=60 // decreases value of n0.val by 60 |
| 10 | Numeric | \*= | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Numeric Multiplication. Multiplies left side with right side with product result placed in left side. n0.val\*=2 is equivalent of n0.val=n0.val\*2 |
| n0.val\*=2 |
| 11 | Numeric | /= | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Numeric Division. Equates division of numerator (left side) and divisor (right side) and places integer quotient in left side. 60000/20001=2 |
| n0.val/=60 |
| 12 | Numeric | %= | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Numeric Modulo. Equates division of numerator (left side) and divisor (right side) and places integer remainder in left side. Divisor MUST be a constant. 60000/20001=19998 |
| n0.val%=60 |

|  |  |  |  |
| --- | --- | --- | --- |
| 13 | Numeric | << | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Arithmetic Bit Shift Left. Moves all bits specified number to the left. Using the 16-bit example that follows, (32-bit uses similar rules) All bits shifted above 15 are **lost** and **undefined**bits become 0 |
| n0.val=n0.val<<4 **0 0 0 0.0 0 1 1.1 1 0 0.0 0 0 1** **0 0 1 1.1 1 0 0.0 0 0 1.** **0 0 1 1.1 1 0 0.0 0 0 1.0 0 0 0** |
| 14 | Numeric | >> | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Arithmetic Bit Shift Right. Moves all bits specified number to the right. Using the 16-bit example that follows, (32-bit uses similar rules) All bits shifted below 0 are **lost** and **undefined**bits become the signed bit. When signed bit is 1 (value is negative) then left filled is with 1’s When signed bit is 0 (value is positive) then left filled is with 0’s |
| n0.val=n0.val>>4 **0 0 0 0.0 0 1 1.1 1 0 0.0 0 0 1** **0 0 0 0.0 0 1 1.1 1 0 0** **0 0 0 0.0 0 0 0.0 0 1 1.1 1 0 0** |
| 15 | Numeric | & | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Logical Bitwise AND. Compares all bits left side to all bits right side(mask) Using the 16-bit example that follows, (32-bit uses similar rules) Result is a bit of 1 where both left and right bits were 1 |
| n0.val=n0.val&35381 **0 1 0 1.1 0 1 1.0 0 1 0.0 1 0 1**n0.val of 23333 **1 0 0 0.1 0 1 0.0 0 1 1.0 1 0 1**mask of 35381 **0 0 0 0.1 0 1 0.0 0 1 0.0 1 0 1**result is 2597 |
| 16 | Numeric | | | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Logical Bitwise OR. Compares all bits left side to all bits right side Using the 16-bit example that follows, (32-bit uses similar rules) Result is a bit of 1 where either left or right bits were 1 |
| n0.val=n0.val|35381 **0 1 0 1.1 0 1 1.0 0 1 0.0 1 0 1**n0.val of 23333 **1 0 0 0.1 0 1 0.0 0 1 1.0 1 0 1**constant 35381 **1 1 0 1.1 0 1 1.0 0 1 1.0 1 0 1**result is 56117 |
| 17 | Numeric | ^ | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Logical Bitwise NOT. Applies bit inversion to all bits in the bitmask Using the 16-bit example that follows, (32-bit uses similar rules) Result is a bit inverted where maskbit was 1, unchanged where maskbit was 0 |
| n0.val=n0.val^35381 **0 1 0 1.1 0 1 1.0 0 1 0.0 1 0 1** n0.val of 23333 **1 0 0 0.1 0 1 0.0 0 1 1.0 1 0 1**bitmask of 35381 **1 1 0 1.0 0 0 1.0 0 1 0.0 0 0 0** result is 53520 |
| 18 | Numeric | == | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Boolean Equality. Evaluate left side to right side. If both left and right sides are the same creates a true condition |
| if(n0.val==va0.val) |
| 19 | Numeric | != | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Boolean Inequality. Evaluate left side to right side. If both left and right sides are different creates a true condition |
| if(n0.val!=va0.val) |
| 20 | Numeric | < | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Boolean Less than. Evaluate left side to right side. If left side is less than right side creates a true condition |
| while(n0.val<va0.val) |
| 21 | Numeric | <= | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Boolean Less than or Equal. Evaluate left side to right side. If left side is less than or equal to right side creates a true condition |
| while(n0.val<=va0.val) |
| 22 | Numeric | > | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Boolean Greater than. Evaluate left side to right side. If left side is greater than right side creates a true condition |
| while(n0.val>va0.val) |

|  |  |  |  |
| --- | --- | --- | --- |
| 23 | Numeric | >= | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Boolean Greater than or Equal. Evaluate left side to right side. If left side is greater than or equal to right side creates a true condition |
| while(n0.val>=va0.val) |
| 24 | Code | { } | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Code Block begins with open brace { on line by itself Code Block ends with closing brace } beginning a new line |
| see if (see [3.25](https://nextion.tech/resource/documents/instruction-set/#s3_if)) while (see [3.26](https://nextion.tech/resource/documents/instruction-set/#s3_while)) and for (see [3.27](https://nextion.tech/resource/documents/instruction-set/#s3_for)) |
| 25 | Code | && | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Condition Joiner AND Conditions may be joined with no spaces between conditions, left to right evaluation |
| see if (see [3.25](https://nextion.tech/resource/documents/instruction-set/#s3_if)) while (see [3.26](https://nextion.tech/resource/documents/instruction-set/#s3_while)) and for (see [3.27](https://nextion.tech/resource/documents/instruction-set/#s3_for)) |
| 26 | Code | || | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Condition Joiner OR Conditions may be joined with no spaces between conditions, left to right evaluation |
| see if (see [3.25](https://nextion.tech/resource/documents/instruction-set/#s3_if)) while (see [3.26](https://nextion.tech/resource/documents/instruction-set/#s3_while)) and for (see [3.27](https://nextion.tech/resource/documents/instruction-set/#s3_for)) |
| 27 | Code | ( ) | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Conditions enclosure begins with open parenthesis ( and ends with closing parenthesis ) at end of line. Parenthesis are not allowed to create complex statements. |
| see if (see [3.25](https://nextion.tech/resource/documents/instruction-set/#s3_if)) while (see [3.26](https://nextion.tech/resource/documents/instruction-set/#s3_while)) and for (see [3.27](https://nextion.tech/resource/documents/instruction-set/#s3_for)) |
| 28 | Code | . | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Period Separator. Separates Page, Component and Attributes Also used with page index and component array. (see [2.29](https://nextion.tech/resource/documents/instruction-set/#s2_29)) |
| page1.va0.val or p0.pic |
| 29 | Code | [ ] | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Array[index]. There are 3 arrays. Keyboard source showcases 2 arrays. The b[.id] component array which takes component .id as index The p[index] page array which takes page index as index These (p[].b[]) need to be used with caution and mindful purpose. Reference to a component without specified Attribute can create for long and potentially frustrating debug sessions. The third array is the Serial Buffer Data u[index] array. This is valid when in active Protocol Reparse mode. Protocol Reparse is an advanced technique that should be skipped if not fully understood. |
| p[pageindex].b[component.id].attribute // global scope b[component.id].attribute // local scope on current page |
| 30 | Comment | // | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Double-Slash Commenting to add user comments to code. Everything to the right of, and including, the double-slash is a comment that will not be executed by the Nextion interpreter. Comments should: 1) occur on a line by themselves with the double-slash at the beginning of the line (no leading spaces), 2) immediately following code on a line without a space separating code and the double slash. Commenting of code blocks should occur: 1) before the condition/iteration 2) inside the opening and closing braces 3) after the code block. *Notes:* It is important to note that comments can not interrupt code blocks without causing an “Error: Index was outside the bounds of the array”. Comments are counted towards the overall “code + attributes” hard limit of 65534. |
| // these are valid comments  sys0=0// reset sys0 to zero  for(sys0=0;sys0<=sys1;sys0++)  // invalid comment between condition/iteration and block |

**3 – Operational Commands**

|  |  |  |  |
| --- | --- | --- | --- |
| No. | Name | Param Count | Description and Usage/Parameters/Examples |
| 1 | page | 1 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Change page to page specified. Unloads old page to load specified page. Nextion loads page 0 by default on power on. usage: page <pid> |
| <pid> is either the page index number, or pagename |
| page 0 // Change page to indexed page 0 page main // Change page to the page named main |
| 2 | ref | 1 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Refresh component (auto-refresh when attribute changes since v0.38) – if component is obstructed (stacking), ref brings component to top. usage: ref <cid> |
| <cid> is component’s .id or .objname attribute of component to refresh – when <cid> is 0 (page component) refreshes all on the current page. |
| ref t0 // Refreshes the component with .objname of t0 ref 3 // Refreshes the component with .id of 3 ref 0 // Refreshes all components on the current page (same as ref 255) |
| 3 | click | 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Trigger the specified components Touch Press/Release Event As event code is always local, object can not be page prefixed usage: click <cid>,<event> |
| <cid> is component’s .id or .objname attribute of component to refresh <event> is 1 to trigger Press Event, 0 to trigger Release Events |
| click b0,1 // Trigger Touch Press Event of component with .objname b0 click 4,0 // Trigger Touch Release Event of component with .id 4 |
| 4 | ref\_stop | 0 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Stops default waveform refreshing (will not refresh when data point added) – waveform refreshing will resume with ref\_star (see [3.5](https://nextion.tech/resource/documents/instruction-set/#s3_ref_star)) usage: ref\_stop |
| ref\_stop // stop refreshing the waveform on each data point added |
| 5 | ref\_star | 0 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Resume default waveform refreshing (refresh on data point add) – used to resume waveform refreshing stopped by ref\_stop (see [3.4](https://nextion.tech/resource/documents/instruction-set/#s3_ref_stop)) usage: ref\_start |
| ref\_star // resume default refreshing, refresh on each data point added |
| 6 | get | 1 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Send attribute/constant over serial (0x70/0x71 Return Data) usage: get <attribute> |
| <attribute> is either numeric value, .txt contents, or constant |
| get t0.txt // sends text contents of t0.txt in 0x70 Return Data format get “123” // sends text constant “123” in 0x70 Return Data format get n0.val // sends numeric value of n0.val in 0x71 Return Data format get 123 // sends numeric constant 123 in 0x71 Return Data format |
| 7 | sendme | 0 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sends number of currently loaded page over serial (0x66 Return Data) – number of currently loaded page is stored in system variable dp – used in a page’s initialize event will auto-send as page loads usage: sendme |
| sendme // sends the value of dp in 0x66 Return Data Format |

|  |  |  |  |
| --- | --- | --- | --- |
| 8 | covx | 4 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Convert variable from numeric type to text, or text to numeric type – text must be text ASCII representation of an integer value. – source and destination types must not be of the same type – when source is numeric, hex format and length not 0 and <4. ie: (len 2) positive significant (byte 0 to 3), 123 = 0000007B = 007B ie: (len 2) negative significant (byte 3 to 0), -123 = FFFFFF85 = FF85 – value is more than allowed space **results in a truncation** – it is recommended to ensure handling source length in user code before covx – in v0.53, covx is deemed undefined if source is larger than length or dest txt\_maxl is smaller than requested length. (some of these undefines, can be exploited) ie: src numeric value of 123 with length 0, result is dest text “123” – when length is fixed and value is less, leading zeros will be added ie: src numeric value of 123 with length 4, result is dest text “0123” – when value is larger than length, .txt truncated to least significant digits ie: src numeric value of 23425 with length 4 result is dest text “3425” usage: covx <src>,<dest>,<length>,<format> |
| <src> is text attribute (or numeric attribute when <dest> is text) <dest> is numeric attribute (or text attribute when <src> is numeric) <length> will determine if leading zeros added to conversion to text <format> 0: integer, 1: Comma separated 1,000s, 2: Hex |
| covx h0.val,t0.txt,0,0 // convert value of h0 into t0.txt without leading zeros covx t0.txt,h0.val,0,0 // convert t0.txt into integer in h0.val <length> ignored. covx h0.val,t0.txt,4,0 // convert value of h0 into t0.txt with exactly 4 digits covx h0.val,t0.txt,4,1 // convert value of h0 into t0.txt with commas covx h0.val,t0.txt,4,2 // convert value of h0 into t0.txt in 2 bytes of hex digits Invalid: covx h0.val,va0.val,0,0 or covx t0.txt,va0.txt,0,0 // src&dest same type. |
| 8a | cov | 3 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png **Depreciated**. Convert from numeric type to text, or text to numeric type – text must be text ASCII representation of an integer value. – source and destination types must not be of the same type – when length is fixed and value is less, leading zeros will be added ie: src numeric value of 123 with length 4, result is dest text “0123” – dest txt\_maxl and length needs be large enough to accommodate conversion. ie: src numeric value of 123 with length 0, result is dest text “123” – when value is larger than length, .txt **results in a truncation** – it is recommended to handle source length in user code before cov **Note:**v0.53 changed behaviour from previous pre v0.53 behaviours. cov is deemed undefined if source is larger than length or the dest txt\_maxl is smaller than the requested length. Some undefines are exploitable. usage: cov <src>,<dest>,<length> |
| <src> is text attribute (or numeric attribute when <dest> is text) <dest> is numeric attribute (or text attribute when <src> is numeric) <length> will determine if leading zeros added to conversion to text |
| cov h0.val,t0.txt,0 // convert value of h0 into t0.txt without leading zeros cov t0.txt,h0.val,0 // convert integer into t0.txt from h0.val <length> ignored. cov h0.val,t0.txt,4 // convert value of h0 into t0.txt with exactly 4 digits Invalid: cov h0.val,va0.val,0 or cov t0.txt,va0.txt,0 // src & dest same type. |
| 9 | touch\_j | 0 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Recalibrate the Resistive Nextion device’s touch sensor – presents 4 points on screen for user to touch, saves, and then reboots. – typically not required as device is calibrated at factory – sensor can be effected by changes of conditions in environment – Capacitive Nextion devices can not be user calibrated. usage: touch\_j |
| touch\_j // trigger the recalibration of touch sensor |

|  |  |  |  |
| --- | --- | --- | --- |
| 10 | substr | 4 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Extract character or characters from contents of a Text attribute usage: substr <src>,<dest>,<start>,<count> |
| <src> is text attribute where text will be extracted from <dest> is text attribute to where extracted text will be placed <start> is start position for extraction (0 is first char, 1 second) <count> is the number of characters to extract |
| substr va0.txt,t0.txt,0,5 // extract first 5 chars from va0.txt, put into t0.txt |
| 11 | vis | 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Hide or Show component on current page – show will refresh component and bring it to the forefront layer – hide will remove component visually, touch events will be disabled – use layering with mindful purpose, can cause ripping and flickering. – use with caution and mindful purpose, may lead to difficult debug session usage: vis <comp><state> |
| <comp> is either .objname or .id of component on current page, – valid .id is 0 – page, 1 to 250 if component exists, and 255 for all <state> is either 0 to hide, or 1 to show. |
| vis b0,0 // hide component with .objname b0 vis b0,1 // show component with .objname b0, refresh on front layer vis 1,0 // hide component with .id 1 vis 1,1 // show component with .id 1, refresh on front layer vis 255,0 // hides all components on the current page |
| 12 | tsw | 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Enable or disable touch events for component on current page – by default, all components are enabled unless disabled by tsw – use with caution and mindful purpose, may lead to difficult debug session usage: tsw <comp><state> |
| <comp> is either .objname or .id of component on current page, – valid .id is 0 – page, 1 to 250 if component exists, and 255 for all <state> is either 0 to disable, or 1 to enable. |
| tsw b0,0 // disable Touch Press/Release events for component b0 tsw b0,1 // enable Touch Press/Release events for component b0 tsw 1,0 // disable Touch Press/Release events for component with id 1 tsw 1,1 // enable Touch Press/Release events for component with id 1 tsw 255,0 // disable all Touch Press/Release events on current page |
| 13 | com\_stop | 0 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Stop execution of instructions received from Serial – Serial will continue to receive and store in buffer. – execution of instructions from Serial will resume with com\_star (see [3.14](https://nextion.tech/resource/documents/instruction-set/#s3_com_star)) – using com\_stop and com\_star may cause a buffer overflow condition. – Refer to device datasheet for buffer size and command queue size usage: com\_stop |
| com\_stop // stops execution of instructions from Serial |
| 14 | com\_star | 0 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Resume execution of instructions received from Serial – used to resume an execution stop caused by com\_stop (see [3.13](https://nextion.tech/resource/documents/instruction-set/#s3_com_stop)) – when com\_star received, all instructions in buffer will be executed – using com\_stop and com\_star may cause a buffer overflow condition. – Refer to device datasheet for buffer size and command queue size usage: com\_star |
| com\_star // resume execution of instruction from Serial |

|  |  |  |  |
| --- | --- | --- | --- |
| 15 | randset | 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Set the Random Generator Range for use with rand (see [6.14](https://nextion.tech/resource/documents/instruction-set/#s6_rand)) – range will persist until changed or Nextion rebooted – set range to desired range before using rand – power on default range is -2147483648 to 2147483647, runtime range is user definable. usage: randset <min>,<max> |
| <min> is value is -2147483648 to 2147483647 <max> is value greater than min and less than 2147483647 |
| randset 1,100 //set current random generator range from 1 to 100 randset 0,65535 //set current random generator range from 0 to 65535 |
| 16 | code\_c | 0 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Clear the commands/data queued in command buffer without execution usage: code\_c |
| code\_c // Clears the command buffer without execution |
| 17 | prints | 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Send raw formatted data over Serial to MCU – prints does not use Nextion Return Data, user must handle MCU side – qty of data may be limited by serial buffer (all data < 1024) – numeric value sent in 4 byte 32-bit little endian order value = byte1+byte2\*256+byte3\*65536+byte4\*16777216 – text content sent is sent 1 ASCII byte per character, without null byte. usage: prints <attr>,<length> |
| <attr> is either component attribute, variable or Constant <length> is either 0 (all) or number to limit the bytes to send. |
| prints t0.txt,0 // return 1 byte per char of t0.txt without null byte ending. prints t0.txt,4 // returns first 4 bytes, 1 byte per char of t0.txt without null byte ending. prints j0.val,0 // return 4 bytes for j0.val in little endian order prints j0.val,1 // returns 1 byte of j0.val in little endian order prints “123”,2 // return 2 bytes for text “12” 0x31 0x32 prints 123,2 // returns 2 bytes for value 123 0x7B 0x00 |
| 17a | print | 1 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png **Depreciated**. Send raw formatted data over Serial to MCU – print/printh does not use Nextion Return Data, user must handle MCU side – qty of data may be limited by serial buffer (all data < 1024) – numeric value sent in 4 byte 32-bit little endian order value = byte1+byte2\*256+byte3\*65536+byte4\*16777216 – text content sent is sent 1 ASCII byte per character, without null byte. usage: print <attr> |
| <attr> is either component attribute, variable or Constant |
| print t0.txt // return 1 byte per char of t0.txt without null byte ending. print j0.val // return 4 bytes for j0.val in little endian order print “123” // return 3 bytes for text “123” 0x31 0x32 0x33 print 123 // return 4 bytes for value 123 0x7B 0x00 0x00 0x00 |
| 18 | printh | 1 to many | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Send raw byte or multiple raw bytes over Serial to MCU – printh is one of the few commands that parameter uses space char 0x20 – when more than one byte is being sent a space separates each byte – byte is represented by 2 of (ASCII char of hexadecimal value per nibble) – qty may be limited by serial buffer (all data < 1024) – print/printh does not use Nextion Return Data, user must handle MCU side usage: printh <hexhex>[<space><hexhex][…<space><hexhex] |
| <hexhex> is hexadecimal value of each nibble. 0x34 as 34 <space> is a space char 0x20, used to separate each <hexhex> pair |
| printh 0d // send single byte: value 13 hex: 0x0d printh 0d 0a // send two bytes: value 13,10 hex: 0x0d0x0a |

|  |  |  |  |
| --- | --- | --- | --- |
| 19 | add | 3 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Add single value to Waveform Channel – waveform channel data range is min 0, max 255 – 1 pixel column is used per data value added – y placement is if value < s0.h then s0.y+s0.h-value, otherwise s0.y usage: add <waveform>,<channel>,<value> |
| <waveform> is the .id of the waveform component <channel> is the channel the data will be added to <value> is ASCII text of data value, or numeric value – valid: va0.val or sys0 or j0.val or 10 |
| add 1,0,30 // add value 30 to Channel 0 of Waveform with .id 1 add 2,1,h0.val // add h0.val to Channel 1 of Waveform with .id 2 |
| 20 | addt | 3 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Add specified number of bytes to Waveform Channel over Serial from MCU – waveform channel data range is min 0, max 255 – 1 pixel column is used per data value added. – addt uses Transparent Data Mode (see [1.16](https://nextion.tech/resource/documents/instruction-set/#s1_16)) – waveform will not refresh until Transparent Data Mode completes. – qty limited by serial buffer (all commands+terminations + data < 1024) – also refer to add command (see [3.19](https://nextion.tech/resource/documents/instruction-set/#s3_add)) usage: add <waveform>,<channel>,<qty> |
| <waveform> is the .id of the waveform component <channel> is the channel the data will be added to <qty> is the number of byte values to add to <channel> |
| addt 2,0,20 // adds 20 bytes to Channel 0 Waveform with .id 2 from serial // byte of data is not ASCII text of byte value, but raw byte of data. |
| 21 | cle | 3 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Clear waveform channel data usage: cle <waveform>,<channel> |
| <waveform> is the .id of the waveform component <channel> is the channel to clear <channel> must be a valid channel: < waveform.ch or 255 0 if .ch 1, 1 if .ch 2, 2 if .ch 3, 3 if .ch=4 and 255 (all channels) |
| cle 1,0 // clear channel 0 data from waveform with .id 1 cle 2,255 // clear all channels from waveform with .id 2 |
| 22 | rest | 0 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Resets the Nextion Device usage: rest |
| rest // immediate reset of Nextion device – reboot. |
| 23 | doevents | 0 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Force immediate screen refresh and receive serial bytes to buffer – useful inside exclusive code block for visual refresh (see [3.26](https://nextion.tech/resource/documents/instruction-set/#s3_while)and [3.27](https://nextion.tech/resource/documents/instruction-set/#s3_for)) usage: doevents |
| doevents // allows refresh and serial to receive during code block |
| 24 | strlen | 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Computes the length of string in <txt> and puts value in <len> usage: strlen <txt>,<len> |
| <txt> must be a string attribute ie: t0.txt, va0.txt <len> must be numeric ie: n0.val, sys0, va0.val |
| strlen t0.txt,n0.val // assigns n0.val with length of t0.txt content |
| 24a | btlen | 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Computes number of bytes string in <txt> uses and puts value in <len> usage: btlen <txt>,<len> |
| <txt> must be a string attribute ie: t0.txt, va0.txt <len> must be numeric ie: n0.val, sys0, va0.val |
| btlen t0.txt,n0.val // assigns n0.val with number of bytes t0.txt occupies |

|  |  |  |  |
| --- | --- | --- | --- |
| 25 | if | Block | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Conditionally execute code block if boolean condition is met – execute commands within block { } if (conditions) is met. – nested conditions using () is not allowed. invalid: ((h0.val+3)>0) – block opening brace { must be on line by itself – no space between block close brace } and else. valid: }else invalid: } else – Text comparison supports ==, != – Numerical comparison supports >, <, ==, !=, >=, <= – conditions can be joined with && or || with no spaces used – nested “if” and “else if” supported. usage: if condition block [else if condition block] [else block] |
| – (conditions) is a simple non-complex boolean comparison evaluating left to right valid: (j0.val>75) invalid: (j0.val+1>75) invalid: (j0.val<now.val+60) |
| if(t0.txt=="123456")  {  page 1  }  if(t0.txt=="123456"||sys0==14&&n0.val==12)  {  page 1  }  if(t0.txt=="123456"&&sys0!=14)  {  page 1  }  if(n0.val==123)  {  b0.txt="stop"  }else  {  b0.txt="start"  }  if(rtc==1)  {  t0.txt="Jan"  }else if(rtc1==2)  {  t0.txt="Feb"  }else if(rtc1==3)  {  t0.txt="Mar"  }else  {  t0.txt="etc"  } |
| 26 | while | Block | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Continually executes code block until boolean condition is no longer met – tests boolean condition and execute commands within block { } if conditions was met and continues to re-execute block until condition is not met. – nested conditions using () is not allowed. invalid: ((h0.val+3)>0) – block opening brace { must be on line by itself – Text comparison supports ==, != – Numerical comparison supports >, <, ==, !=, >=, <= – conditions can be joined with && or || with no spaces used – block runs exclusively until completion unless doevents used (see [3.23](https://nextion.tech/resource/documents/instruction-set/#s3_doevents)) usage: while condition block |
| – (conditions) is a simple non-complex boolean comparison evaluating left to right valid: (j0.val>75) invalid: (j0.val+1>75) |
| // increment n0.val as lon as n0.val < 100. result: b0.val=100  // will not visually see n0.val increment, refresh when while-loop completes  while(n0.val<100)  {  n0.val++  }  //increment n0.val as long as n0.val < 100. result: n0.val=100  // will visually see n0.val increment, refresh each evaluation of while-loop  while(n0.val<100)  {  n0.val++  doevents  } |

|  |  |  |  |
| --- | --- | --- | --- |
| 27 | for | Block | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Iterate execution of code block as long as boolean condition is met – executes init\_assignment, then tests boolean condition and executes commands within block { } if boolean condition is met, when iteration of block execution completes step\_assignment is executed. Continues to iterate block and step\_assignment until boolean condition is not met. – nested conditions using () is not allowed. invalid: ((h0.val+3)>0) – block opening brace { must be on line by itself – Text comparison supports ==, != – Numerical comparison supports >, <, ==, !=, >=, <= – conditions can be joined with && or || with no spaces used – block runs exclusively until completion unless doevents used (see [3.23](https://nextion.tech/resource/documents/instruction-set/#s3_doevents)) usage: for(init\_assignment;condition;step\_assignment) block |
| – init\_assignment and step\_assignment are simple non-complex statement valid: n0.val=4, sys2++, n0.val=sys2\*4+3 invalid: n0.val=3+(sys2\*4)-1 – (conditions) is a simple non-complex boolean comparison evaluating left to right valid: (j0.val>75) invalid: (j0.val+1>75) |
| // iterate n0.val by 1's as long as n0.val<100. result: n0.val=100  // will not visually see n0val increment until for-loop completes  for(n0.val=0;n0.val<100;n0.val++)  {  }  ////iterate n0.val by 2's as long as n0.val<100. result: n0.val=100  // will visually see n0.val increment when doevents processed  for(n0.val=0;n0.val<100;n0.val+=2)  {  doevents  } |

|  |  |  |  |
| --- | --- | --- | --- |
| 28 | wepo | 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sKP.png Store value/string to EEPROM – EEPROM valid address range is from 0 to 1023 (1K EEPROM) – numeric value length: is 4 bytes, -2147483648 to 2147483647 – numeric data type signed long integer, stored in little endian order. val[addr+3]\*16777216+val[addr+2]\*65536+val[addr+1]\*256+val[addr] – string content length: .txt content is .txt-maxl +1, or constant length +1 usage: wepo <attr>,<addr> |
| <attr> is variable or constant <addr> is storage starting address in EEPROM |
| wepo t0.txt,10 // writes t0.txt contents in addresses 10 to 10+t0.txt-maxl wepo “abcd”,10 // write constant “abcd” in addresses 10 to 14 wepo 11,10 // write constant 11 in addresses 10 to 13 wepo n0.val,10 // write value n0.val in addresses 10 to 13 |
| 29 | repo | 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sKP.png Read value from EEPROM – EEPROM valid address range is from 0 to 1023 (1K EEPROM) – numeric value length: is 4 bytes, -2147483648 to 2147483647 – numeric data type signed long integer, stored in little endian order. val[addr+3]\*16777216+val[addr+2]\*65536+val[addr+1]\*256+val[addr] – string content length: .txt content is lesser of .txt-maxl or until null reached. usage: repo <attr>,<addr> |
| <attr> is variable or constant <addr> is storage starting address in EEPROM |
| repo t0.txt,10 // reads qty .txt-maxl chars (or until null) from 10 into t0.txt repo n0.val,10 // reads 4 bytes from address 10 to 13 into n0.val |
| 30 | wept | 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sKP.png Store specified number of bytes to EEPROM over Serial from MCU – EEPROM valid address range is from 0 to 1023 (1K EEPROM) – wept uses Transparent Data Mode (see [1.16](https://nextion.tech/resource/documents/instruction-set/#s1_16)) – qty limited by serial buffer (all commands+terminations + data < 1024) usage: wept <addr>,<qty> |
| <addr> is storage starting address in EEPROM <qty> is the number of bytes to store |
| wept 30,20 // writes 20 bytes into EEPROM addresses 30 to 49 from serial // byte of data is not ASCII text of byte value, but raw byte of data. |
| 31 | rept | 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sKP.png Read specified number of bytes from EEPROM over Serial to MCU – EEPROM valid address range is from 0 to 1023 (1K EEPROM) usage: rept <addr>,<qty> |
| <addr> is storage starting address in EEPROM <qty> is the number of bytes to read |
| rept 30,20 // sends 20 bytes from EEPROM addresses 30 to 49 to serial // byte of data is not ASCII text of byte value, but raw byte of data. |
| 32 | cfgpio | 3 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sKP.png Configure Nextion GPIO usage: cfgpio <io><mode><comp> |
| <io> is the number of the extended I/O pin. – Valid values in PWM output mode: 4 to 7, all other modes 0 to 7. <mode> is the working mode of pin selected by <io>. – Valid values: 0-pull up input, 1-input binding, 2-push pull output, 3-PWM output, 4-open drain output. <comp> component .objname or .id when <mode> is 1 (otherwise use 0) – in binding mode, cfgpio needs to be declared after every refresh of page to reconnect to Touch event, best to put cfgpio in page pre-initialization event |
| cfgpio 0,0,0 // configures io0 as a pull-up input. Read as n0.val=pio0. cfgpio 1,2,0 // configures io1 as a push-pull output, write as pio1=1 cfgpio 2,1, b0 // configures io2 as binding input with current page b0. // binding triggers b0 Press on falling edge and b0 Release on rising edge For PWM mode, set duty cycle before cfgpio: ie: pwm4=20 for 20% duty. cfgpio 4,3,0 // configures io4 as PWM output. pwmf=933 to change Hz. // changing pwmf changes frequency of all configured PWM io4 to io7 |
| 33 | ucopy | 4 | **https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Advanced**. Read Only. Valid in active Protocol Reparse mode. Copies data from the serial buffer. When Nextion is in active Protocol Reparse mode, ucopy copies data from the serial buffer. Most HMI applications will not require Protocol Reparse and should be skipped if not fully understood. usage: ucopy <attr>,<srcstart>,<len>,<deststart> |
| <attr> must be a writeable attribute ie: t0.txt, va0.val <srcstart> must be numeric value ie: 0 <len> must be a numeric value ie: 4 <deststart> must be numeric value ie: 0 |
| ucopy n0.val,0,2,0 // copy buffer bytes 0,1 to lower 2 bytes of n0.val ucopy n0.val,0,2,2 // copy buffer bytes 0,1 to upper 2 bytes of n0.val ucopy n0.val,0,4,0 // copy buffer bytes 0,1,2,4 to n0.val ucopy t0.txt,0,10,0 // copy buffer bytes 0 to 9 into t0.txt |
| 34 | move | 7 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png Move component. usage: move <comp>,<x1>,<y1>,<x2>,<y2>,<priority>,<time> |
| <comp> is the component name or component id <x1> is the starting X coordinate <y1> is the starting Y coordinate <x2> is the destination X coordinate <y2> is the destination Y coordinate <priority> is a value 0 to 100, 100 being highest priority <time> is time in ms. |
| move t0,-30,-30,100,150,95,120 // 120ms to move t0 into position 100,150 move t1,-30,-30,200,150,90,180 // 180ms to move t1 into position 200,150 move t2,-30,-30,300,150,100,150 // 150ms to move t2 into position 300,150 // given the example priorities, t2 moves first, then t0 and lastly t1 |
| 35 | play | 3 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png Play audio resource on selected Channel usage: play <ch>,<resource>,<loop> |
| <ch> is the component name or component id <resource> is the Audio Resource ID <loop> is 0 for no looping, 1 to loopthe starting Y coordinate Notes: The play instruction is used to configure and start audio playback. audio0 and audio1 are used to control the channel. Audio playback is global and playback continues after leaving and changing pages, if you want the audio to stop on leaving the page, you should do so in the page leave event |
| play 1,3,0// play resource 3 on channel 1 with no looping play 0,2,1// play resource 2 on channel 0 with looping |
| 36 | twfile | 2 | **https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png Advanced**. Transfer file over Serial usage: twfile <filepath>,<filesize> |
| <filepath> is destination path and filename quote encapsulated text <filesize> is the size of the file in bytes. Note: current support is file in root. Subdirectories are not supported. |
| twfile “ram/0.jpg”,1120// transfer jpg over serial to ram/0.jpg size 1120 bytes twfile “sd0/0.jpg”,1120// transfer jpg over serial to sd0/0.jpg size 1120 bytes |
| 37 | delfile | 1 | **https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png Advanced**. Delete external file. usage: delfile <filepath> |
| <filepath> is target path and filename as quote encapsulated text Note: current support is file in root. Subdirectories are not supported. |
| delfile “ram/0.jpg”// remove transferred file ram/0.jpg delfile “sd0/0.jpg”// remove transferred file sd0/0.jpg |

|  |  |  |  |
| --- | --- | --- | --- |
| 38 | refile | 2 | **https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png Advanced**. Rename external file. usage: refile <oldname>,<newname> |
| <oldname> is source path and filename as quote encapsulated text <newname> is target path and filename as quote encapsulated text Note: current support is file in root. Subdirectories are not supported. |
| refile “ram/0.jpg”,”ram/1.jpg”// rename file ram/0.jpg to ram/1.jpg refile “sd0/0.jpg”,”sd0/1.jpg”// rename file sd0/0.jpg to sd0/1.jpg |
| 39 | findfile | 2 | **https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png Advanced**. Find File reports if named external file exists usage: findfile <pathfile>,<result> |
| <pathfile> is source path and filename as quote encapsulated text <result> is a numeric attribute for the result to be stored Returns 0 result if find fails, returns 1 if find is successful. Note: current support is file in root. Subdirectories are not supported. |
| findfile “ram/0.jpg”,n0.val// check if file exists, store result in n0.val findfile “sd0/0.jpg”,sys0//check if file exists, store result in sys0 |
| 40 | rdfile | 4 | **https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png Advanced**. Read File contents and outputs contents over serial usage: rdfile <pathfile>,<offset>,<count>,<crc> |
| <pathfile> is source path and filename as quote encapsulated text <offset> is the starting offset of the file <count> is number of bytes to return (see note if 0) <crc> is an option (0: no crc, 1: Modbus crc16, 10: crc32) Note: current support is file in root. Subdirectories are not supported. If count is 0, then 4 byte file size is returned in little endian order. |
| rdfile “ram/0.jpg”,0,10,0// send first 10 bytes of file, no CRC, 10 bytes. rdfile “sd0/0.jpg”,0,10,1// send first 10 bytes of file, MODBUS CRC, 12 bytes. rdfile “sd0/0.jpg”,0,10,10// send first 10 bytes of file, CRC32, 14 bytes. |
| 41 | setlayer | 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png Set Component Layer usage: setlayer <comp1>,<comp2> |
| <comp1> is component ID or objname of component needing to change layers <comp2> is the component ID or object name comp1 is placed above Note: using comp2 value of 255 places comp1 on topmost layer. |
| setlayer t0,n0//places to above n0’s layer setlayer t0,255//place t0 on the topmost layer setlayer n0,3//place n0 on the 3rd layer |

**4 – GUI Designing Commands**

|  |  |  |  |
| --- | --- | --- | --- |
| No. | Name | Param Count | Description and Usage/Parameters/Examples |
| 1 | cls | 1 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Clear the screen and fill the entire screen with specified color usage: cls <color> |
| <color> is either decimal 565 Color Value or Color Constant |
| cls BLUE // Clear the screen and fill with color BLUE cls 1024 // Clear the screen and fill with color 1024 |
| 2 | pic | 3 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Display a Resource Picture at specified coordinate usage: pic <x>,<y>,<picid> |
| <x> is the x coordinate of upper left corner where picture should be drawn <y> is the y coordinate of upper left corner where picture should be drawn <picid> is the number of the Resource Picture in the HMI design |
| pic 10,20,0 // Display Resource Picture #0 with upper left corner at (10,20) pic 40,50,1 // Display Resource Picture #1 with upper left corner at (40,50) |
| 3 | picq | 5 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Crop Picture area from Resource Picture using defined area – replaces defined area with content from the same area of Resource Picture – Resource Picture should be full screen-size or area might be undefined usage: picq <x>,<y>,<w>,<h>,<picid> |
| <x> is the x coordinate of upper left corner of defined crop area <y> is the y coordinate of upper left corner of defined crop area <w> is the width of the defined crop area <h> is the height of the defined crop area <picid> is the number of the Resource Picture in the HMI design |
| picq 20,50,30,20,0 // crops area 30×20, from (20,50) to (49,69), from Resource Picture 0 |
| 4 | xpic | 7 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Advanced Crop Picture crop area from source Resource Picture render at destination coordinate usage: xpic <destx>,<desty>,<w>,<h>,<srcx>,<srcy>,<picid> |
| <destx> is the x coordinate of destination upper left corner <desty> is the y coordinate of destination upper left corner <w> is the width of the defined crop area <h> is the height of the defined crop area <srcx> is the x coordinate of upper left corner of defined crop area <srcy> is the y coordinate of upper left corner of defined crop area <picid> is the number of the Resource Picture in the HMI design |
| xpic 20,50,30,20,15,15,0 // crops area 30×20, from (15,15) to (44,34), // from Resource Picture 0 and renders it with upper left corner at (20,50) |
| 5 | xstr | 11 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Prints text on the Nextion device using defined area for text rendering usage: xstr <x>,<y>,<w>,<h>,<font>,<pco>,<bco>,<xcen>,<ycen>,<sta>,<text> |
| <x> is the x coordinate of upper left corner of defined text area <y> is the y coordinate of upper left corner of defined text area <w> is the width of the defined text area <h> is the height of the defined text area <font> is the number of the Resource Font <pco> is the foreground color of text (Color Constant or 565 color value) <bco> is a) background color of text, or b) picid if <sta> is set to 0 or 2 <xcen> is the Horizontal Alignment (0 – left, 1 – centered, 2 – right) <ycen> is the Vertical Alignment (0 – top/upper, 1 – center, 3 – bottom/lower) <sta> is background Fill (0 – crop image, 1 – solid color, 2 – image, 3 – none) <text> is the string content (constant or .txt attribute), ie “China”, or va0.txt |
| xstr 10,10,100,30,1,WHITE,GREEN,1,1,1,va0.txt // use are 100×30 from (10,10) to (109,39) to print contents of va0.txt using // Font Resource 1 rendering Green letters on White background with both // horizontal and vertical centering and sta set as solid-color. |
| 6 | fill | 5 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Fill a defined area with specified color usage: fill <x>,<y>,<w>,<h>,<color> |
| <x> is the x coordinate of upper left corner of defined fill area <y> is the y coordinate of upper left corner of defined fill area <w> is the width of the defined fill area <h> is the height of the defined fill area <color> is fill color, either decimal 565 Color Value or Color Constant |
| fill 20,20,150,50,1024 // fills area 150×50 from (20,20) to (169,69) with 565 Color 1024. |
| 7 | line | 5 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Draw a line from point to point with specified color usage: line <x1>,<y1>,<x2>,<y2>,<color> |
| <x1> is the x coordinate of the starting point of the line to be drawn <y1> is the y coordinate of the starting point of the line to be drawn <x2> is the x coordinate of the ending point of the line to be drawn <y2> is the y coordinate of the ending point of the line to be drawn <color> is line color, either decimal 565 Color Value or Color Constant |
| line 20,30,170,200,BLUE // draws line in BLUE from (20,30) to (170,200) |
| 8 | draw | 5 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Draw a hollow rectangle around specified area with specified color usage: draw <x1>,<y1>,<x2>,<y2>,<color> |
| <x1> is the x coordinate of the upper left corner of rectangle area <y1> is the y coordinate of the upper left corner of rectangle area <x2> is the x coordinate of the lower right corner of rectangle area <y2> is the y coordinate of the lower right corner of rectangle area <color> is line color, either decimal 565 Color Value or Color Constant |
| draw 10,10,70,70,GREEN // draw a Green rectangle around (10,10) to (79,79) // effectively four lines from (x1,y1) to (x2,y1) to (x2,y2) to (x1,y2) to (x1,y1) |
| 9 | cir | 4 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Draw a hollow circle with specified radius and specified color usage: cir <x>,<y>,<radius>,<color> |
| <x> is the x coordinate of the center point for the circle <y> is the y coordinate of the center point for the circle <radius> is the radius in pixels <color> is line color, either decimal 565 Color Value or Color Constant |
| cir 100,100,30,RED // renders a hollow Red circle with circle center at (100,100), // a 30 pixel radius, a 61 pixel diameter, within boundary (70,70) to (130,130). |
| 10 | cirs | 4 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Draw a filled circle with specified radius and specified color usage: cirs <x>,<y>,<radius>,<color> |
| <x> is the x coordinate of the center point for the circle <y> is the y coordinate of the center point for the circle <radius> is the radius in pixels <color> is fill color, either decimal 565 Color Value or Color Constant |
| cir 100,100,30,RED // renders a filled Red circle with center at (100,100), // a 30 pixel radius, a 61 pixel diameter, within boundary (70,70) to (130,130). |

**5 – Color Code Constants**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| No. | Constant | 565 Color Value | Indicator Color |  |
| 1 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png BLACK | 0 | Black |  |
| 2 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png BLUE | 31 | Blue |  |
| 3 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png BROWN | 48192 | Brown |  |
| 4 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png GREEN | 2016 | Green |  |
| 5 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png YELLOW | 65504 | Yellow |  |
| 6 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png RED | 63488 | Red |  |
| 7 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png GRAY | 33840 | Gray |  |
| 8 | https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png WHITE | 65535 | White |  |
| Note: | 16-bit 565 Colors are in decimal values from 0 to 65535 24-bit RGB **11011000 11011000 11011000** 16-bit 565 **11011 110110 11011** | | | |

**6 – System Variables**

|  |  |  |  |
| --- | --- | --- | --- |
| No. | Name | Meaning | Example/Description |
| 1 | dp | Current Page ID | dp=1, n0.val=dp |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png read: Contains the current page displayed as per the HMI design write: change page to value specified (same effect as page command) min 0, max # of highest existing page in the user’s HMI design. |
| 2 | dim dims | Nextion Backlight | dim=32, dims=100 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sets the backlight level in percent min 0, max 100, **default** 100 or user defined Note: dim=32 will set the current backlight level to 32%. using dims=32 will set the current backlight level to 32% and save this to be new power on default backlight level, persisting until changed. |
| 3 | baud bauds | Nextion Baud Rate | baud=9600, bauds=9600 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sets the Nextion Baud rate in bits-per-second min 2400, max 921600, **default** 9600 or user defined Valid values are: 2400, 4800, 9600, 19200, 38400, 57600, and 115200, 230400, 256000, 512000, and 921600 Note: baud=38400 will set the current baud rate to 38400 using bauds=38400 will set the current baud rate to 38400 and save this to be new power on default baud rate, persisting until changed. Note: on rare occasions bauds has become lost. It is recommended to specify bauds=9600 in the first page’s Preinitialization Event of HMI. |
| 4 | spax spay | Font Spacing | spax=2, spay=2 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sets the default rendering space for xstr: horizontally between font characters with spax additional pixels and vertically between rows (if multi-lined) with spay additional pixels. min 0, max 65535, **default** 0 Note: Components now have their own individual .spax/.spay attributes that are now used to determine spacing for the individual component. |
| 5 | thc | Touch Draw Brush Color | thc=RED, thc=1024 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sets the Touch Drawing brush color min 0, max 65535, **default** 0 Valid choices are either color constants or the decimal 565 color value. |
| 6 | thdra | Touch Drawing | thdra=1 (on), thdra=0 (off) |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Turns the internal drawing function on or off. min 0, max 1, **default** 0 When the drawing function is on, Nextion will follow touch dragging with the current brush color (as determined by the thc variable). |

|  |  |  |  |
| --- | --- | --- | --- |
| 7 | ussp | Sleep on No Serial | ussp=30 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sets internal No-serial-then-sleep timer to specified value in seconds min 3, max 65535, **default** 0 (max: 18 hours 12 minutes 15 seconds) Nextion will auto-enter sleep mode if and when this timer expires. Note: Nextion device needs to exit sleep to issue ussp=0 to disable sleep on no serial, otherwise once ussp is set, it will persist until reboot or reset. |
| 8 | thsp | Sleep on No Touch | thsp=30 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sets internal No-touch-then-sleep timer to specified value in seconds min 3, max 65535, **default** 0 (max: 18 hours 12 minutes 15 seconds) Nextion will auto-enter sleep mode if and when this timer expires. Note: Nextion device needs to exit sleep to issue thsp=0 to disable sleep on no touch, otherwise once thsp is set, it will persist until reboot or reset. |
| 9 | thup | Auto Wake on Touch | thup=0 (do not wake), thup=1 (wake on touch) |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sets if Nextion should auto-wake from sleep when touch press occurs. min 0, max 1, **default** 0 When value is 1 and Nextion is in sleep mode, the first touch will only trigger the auto wake mode and not trigger a Touch Event. thup has no influence on sendxy, sendxy will operate independently. |
| 10 | sendxy | RealTime Touch Coordinates | sendxy=1 (start sending) sendxy=0 (stop sending) |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sets if Nextion should send 0x67 and 0x68 Return Data min 0, max 1, **default** 0 – Less accurate closer to edges, and more accurate closer to center. Note: expecting exact pixel (0,0) or (799,479) is simply not achievable. |
| 11 | delay | Delay | delay=100 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Creates a halt in Nextion code execution for specified time in ms min 0, max 65535 As delay is interpreted, a total halt is avoided. Incoming serial data is received and stored in buffer but not be processed until delay ends. If delay of more than 65.535 seconds is required, use of multiple delay statements required. delay=-1 is max. 65.535 seconds. |
| 12 | sleep | Sleep | sleep=1 (Enter sleep mode) or sleep=0 (Exit sleep mode) |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sets Nextion mode between sleep and awake. min 0, max 1, or **default** 0 When exiting sleep mode, the Nextion device will auto refresh the page (as determined by the value in the wup variable) and reset the backlight brightness (as determined by the value in the dim variable). A get/print/printh/wup/sleep instruction can be executed during sleep mode. Extended IO binding interrupts do not occur in sleep. |
| 13 | bkcmd | Pass / Fail Return Data | bkcmd=3 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sets the level of Return Data on commands processed over Serial. min 0, max 3, **default** 2 – Level 0 is Off – no pass/fail will be returned – Level 1 is OnSuccess, only when last serial command successful. – Level 2 is OnFailure, only when last serial command failed – Level 3 is Always, returns 0x00 to 0x23 result of serial command. Result is only sent after serial command/task has been completed, as such this provides an invaluable status for debugging and branching. Table 2 of Section 7 Nextion Return Data is not subject to bkcmd |
| 14 | rand | Random Value | n0.val=rand |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Readonly. Value returned by rand is random every time it is referred to. **default** range is 0 to 4294967295 range of rand is user customizable using the randset command range as set with randset will persist until reboot or reset |

|  |  |  |  |
| --- | --- | --- | --- |
| 15 | sys0 sys1 sys2 | Numeric System Variables | sys0=10 sys1=40 sys2=60 n0.val=sys2 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png System Variables are global in nature with no need to define or create. They can be read or written from any page. 32-bit unsigned integers. min value of 0, max value of 4294967295 Suggested uses of sys variables include – as temporary variables in complex calculations – as parameters to pass to click function or pass between pages. |
| 16 | wup | Wake Up Page | wup=2, n0.val=wup |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sets which page Nextion loads when exiting sleep mode min is 0, max is # of last page in HMI, or **default** 255 When wup=255 (not set to any existing page) – Nextion wakes up to current page, refreshing components only wup can be set even when Nextion is in sleep mode |
| 17 | usup | Wake On Serial Data | usup=0, usup=1 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Sets if serial data wakes Nextion from sleep mode automatically. min is 0, max is 1, **default**0 When usup=0, send sleep=0ÿÿÿ to wake Nextion When usup=1, any serial received wakes Nextion |
| 18 | rtc0 rtc1 rtc2 rtc3 rtc4 rtc5 rtc6 | RTC | rtc0=2017, rtc1=8, rtc2=28, rtc3=16, rtc4=50, rtc5=36, n0.val=rtc6 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sKP.png Nextion RTC: rtc0 is year 2000 to 2099, rtc1 is month 1 to 12, rtc2 is day 1 to 31, rtc3 is hour 0 to 23, rtc4 is minute 0 to 59, rtc5 is second 0 to 59. rtc6 is dayofweek 0 to 6 (Sunday=0, Saturday=6) rtc6 is readonly and calculated by RTC when date is valid. |
| 19 | pio0 pio1 pio2 pio3 pio4 pio5 pio6 pio7 | GPIO | pio3=1, pio3=0, n0.val=pio3 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sKP.png Default mode when power on: pull up input mode Internal pull up resistor: 50K GPIO is digital. Value of 0 or 1 only. – refer to cfgpio command for setting GPIO mode read if in input mode, write if in output mode |
| 19 | pwm4 pwm5 pwm6 pwm7 | PWM Duty Cycle | pwm7=25 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sKP.png Value in percentage. min 0, max 100, **default**50. – refer to cfgpio command for setting GPIO mode https://cdn.nextion.tech/wp-content/uploads/2019/07/sK.png supports pwm4, pwm5, pwm6 and pwm7 https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png supports only pwm6 and pwm7 |
| 21 | pwmf | PWM Frequency | pwmf=933 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sKP.png Value is in Hz. min value 1 Hz, max value 65535 Hz. **default**1000 Hz All PWM output is unified to only one Frequency, no independent individual settings are allowed. – refer to cfgpio command for setting GPIO mode |
| 22 | addr | Address | addr=257 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png**Advanced**. Enables/disables Nextion’s two byte Address Mode 0, or min value 256, max value 2815. **default**0 Setting addr will persist to be the new power-on default. – refer to section [1.19](https://nextion.tech/resource/documents/instruction-set/#s1_16) |
| 23 | tch0 tch1 tch2 tch3 | Touch Coordinates | x.val=tch0, y.val=tch1 |
| https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Readonly. When Pressed tch0 is x coordinate, tch1 is y coordinate. When released (not currently pressed), tch0 and tch1 will be 0. tch2 holds the last x coordinate, tch3 holds the last y coordinate. |

|  |  |  |  |
| --- | --- | --- | --- |
| 24 | recmod | Protocol Reparse | recmod=0, recmod=1 |
| **https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Advanced**. Set passive or active Protocol Reparse mode. min is 0, max is 1, **default**0 When recmod=0, Nextion is in passive mode and processes serial data according to the Nextion Instruction Set, this is the default power on processing. When recmod=1, Nextion enters into active mode where the serial data waits to be processed by event code. Most HMI applications will not require Protocol Reparse and should be skipped if not fully understood. |
| 25 | usize | Bytes in Serial Buffer | n0.val=usize |
| **https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Advanced**. Read Only. Valid in active Protocol Reparse mode. min is 0, max is 1024 When Nextion is in active Protocol Reparse mode, usize reports the number of available bytes in the serial buffer. Most HMI applications will not require Protocol Reparse and should be skipped if not fully understood. |
| 26 | u[index] | Serial Buffer Data | n0.val=u[0] |
| **https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png Advanced**. Read Only. Valid in active Protocol Reparse mode. min is 0, max is 255 When Nextion is in active Protocol Reparse mode, the u[index] array returns the byte at position index from the serial buffer. Most HMI applications will not require Protocol Reparse and should be skipped if not fully understood. |
| 27 | eql eqm eqh | Equalizer Groupings | eqm=7 |
| **https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png**Valid on Nextion Device, not supported in Debug Simulator. min is 0, max is 15 eql: Bass (31Hz to 125Hz, eq0..eq2) eqm: Midrange (250Hz to 2000Hz, eq3..eq6) eqh: Treble (4000Hz to 1600Hz, eq7..eq9) Setting to 7 is Balanced with no attenuation, no gain Setting 0..6, the lower the value the higher the attenuation Setting 8..15, the higher the value the higher the gain NOTE: The base of the equalizer is operated according to eq0..eq9, when a group is modified the corresponding individual bands are modified, however modifying an individual band does not modify the group. (ie: setting eql=4 sets eq0, eq1 and eq2 to 4, but setting eq1=3 does not modify eql to 3, eq0 and eq2 remain at 4). |
| 28 | eq0 eq1 eq2 eq3 eq4 eq5 eq6 eq7 eq8 eq9 | Equalizer Individual Bands | eq6=7 |
| **https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png**Valid on Nextion Device, not supported in Debug Simulator. min is 0, max is 15 eq0 (31Hz), eq1 (62Hz), eq2 (125Hz), eq3 (250Hz), eq4 (500Hz), eq5 (1000Hz), eq6 (2000Hz), eq7 (4000Hz), eq8 (8000Hz), eq9 (16000Hz) Setting to 7 is Balanced with no attenuation, no gain Setting 0..6, the lower the value the higher the attenuation Setting 8..15, the higher the value the higher the gain NOTE: The base of the equalizer is operated according to eq0..eq9, when a group is modified the corresponding individual bands are modified, however modifying an individual band does not modify the group. (ie: setting eql=4 sets eq0, eq1 and eq2 to 4, but setting eq1=3 does not modify eql to 3, eq0 and eq2 remain at 4). |
| 29 | volume | Audio Volume | volume=60 |
| **https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png**Valid on Nextion Device, not supported in Debug Simulator. min is 0, max is 100 volume persists and sets the power-on default setting for the audio volume |
| 30 | audio0 audio1 | Audio Channel Control | audio0=0// stop channel 0 audio playback |
| **https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png** min is 0, max is 2 0 (stop), 1 (resume), 2 (pause). Notes: The play instruction is used to configure and start audio playback. audio0 and audio1 are only used to control the channel. Only if the channel is paused can it be resumed, if the channel is stopped then the play instruction is required to start it again. Audio playback is global and playback continues after leaving and changing pages, if you want the channel to stop on leaving the page, you must do so in the page leave event |

**7 – Format of Nextion Return Data**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Return Codes dependent on bkcmd value being greater than 0** | | | | | |
| No. | Byte | bkcmd | len | Meaning | Format/Description |
| 1 | 0x00 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Invalid Instruction | 0x00 0xFF 0xFF 0xFF |
| Returned when instruction sent by user has failed |
| 2 | 0x01 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 1,3 | 4 | Instruction Successful | 0x01 0xFF 0xFF 0xFF |
| Returned when instruction sent by user was successful |
| 3 | 0x02 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Invalid Component ID | 0x02 0xFF 0xFF 0xFF |
| Returned when invalid Component ID or name was used |
| 4 | 0x03 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Invalid Page ID | 0x03 0xFF 0xFF 0xFF |
| Returned when invalid Page ID or name was used |
| 5 | 0x04 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Invalid Picture ID | 0x04 0xFF 0xFF 0xFF |
| Returned when invalid Picture ID was used |
| 6 | 0x05 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Invalid Font ID | 0x05 0xFF 0xFF 0xFF |
| Returned when invalid Font ID was used |
| 7 | 0x06 https://cdn.nextion.tech/wp-content/uploads/2019/07/sP.png | 2,3 | 4 | Invalid File Operation | 0x06 0xFF 0xFF 0xFF |
| Returned when File operation fails |
| 8 | 0x09 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Invalid CRC | 0x09 0xFF 0xFF 0xFF |
| Returned when Instructions with CRC validation fails their CRC check |
| 9 | 0x11 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Invalid Baud rate Setting | 0x11 0xFF 0xFF 0xFF |
| Returned when invalid Baud rate was used |
| 10 | 0x12 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Invalid Waveform ID or Channel # | 0x12 0xFF 0xFF 0xFF |
| Returned when invalid Waveform ID or Channel # was used |
| 11 | 0x1A https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Invalid Variable name or attribute | 0x1A 0xFF 0xFF 0xFF |
| Returned when invalid Variable name or invalid attribute was used |
| 12 | 0x1B https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Invalid Variable Operation | 0x1B 0xFF 0xFF 0xFF |
| Returned when Operation of Variable is invalid. ie: Text assignment t0.txt=abc or t0.txt=23, Numeric assignment j0.val=”50″ or j0.val=abc |
| 13 | 0x1C https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Assignment failed to assign | 0x1C 0xFF 0xFF 0xFF |
| Returned when attribute assignment failed to assign |
| 14 | 0x1D https://cdn.nextion.tech/wp-content/uploads/2019/07/sKP.png | 2,3 | 4 | EEPROM Operation failed | 0x1D 0xFF 0xFF 0xFF |
| Returned when an EEPROM Operation has failed |
| 15 | 0x1E https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Invalid Quantity of Parameters | 0x1E 0xFF 0xFF 0xFF |
| Returned when the number of instruction parameters is invalid |
| 16 | 0x1F https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | IO Operation failed | 0x1F 0xFF 0xFF 0xFF |
| Returned when an IO operation has failed |
| 17 | 0x20 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Escape Character Invalid | 0x20 0xFF 0xFF 0xFF |
| Returned when an unsupported escape character is used |
| 18 | 0x23 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 2,3 | 4 | Variable name too long | 0x23 0xFF 0xFF 0xFF |
| Returned when variable name is too long. Max length is 29 characters: 14 for page + “.” + 14 for component. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Return Codes not affected by bkcmd value, valid in all cases** | | | | |
| No. | Byte | length | Meaning | Format/Description |
| 19 | 0x00 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 6 | Nextion Startup | 0x00 0x00 0x00 0xFF 0xFF 0xFF |
| Returned when Nextion has started or reset |
| 20 | 0x24 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 4 | Serial Buffer Overflow | 0x24 0xFF 0xFF 0xFF |
| Returned when a Serial Buffer overflow occurs Buffer will continue to receive the current instruction, all previous instructions are lost. |
| 21 | 0x65 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 7 | Touch Event | 0x65 0x00 0x01 0x01 0xFF 0xFF 0xFF |
| Returned when Touch occurs and component’s corresponding Send Component ID is checked in the users HMI design. 0x00 is page number, 0x01 is component ID, 0x01 is event (0x01 Press and 0x00 Release) |
| **data**: Page 0, Component 1, Pressed |
| 22 | 0x66 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 5 | Current Page Number | 0x66 0x01 0xFF 0xFF 0xFF |
| Returned when the sendme command is used. 0x01 is current page number |
| **data**: page 1 |
| 23 | 0x67 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 9 | Touch Coordinate (awake) | 0x67 0x00 0x7A 0x00 0x1E 0x01 0xFF 0xFF 0xFF |
| Returned when sendxy=1 and not in sleep mode 0x00 0x7A is x coordinate in big endian order, 0x00 0x1E is y coordinate in big endian order, 0x01 is event (0x01 Press and 0x00 Release) |
| (0x00\*256+0x71,0x00\*256+0x1E) |
| **data**: (122,30) Pressed |
| 24 | 0x68 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 9 | Touch Coordinate (sleep) | 0x68 0x00 0x7A 0x00 0x1E 0x01 0xFF 0xFF 0xFF |
| Returned when sendxy=1 and in sleep mode 0x00 0x7A is x coordinate in big endian order, 0x00 0x1E is y coordinate in big endian order, 0x01 is event (0x01 Press and 0x00 Release) |
| (0x00\*256+0x71,0x00\*256+0x1E) |
| **data**: (122,30) Pressed |
| 25 | 0x70 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | Varied | String Data Enclosed | 0x70 0x61 0x62 0x31 0x32 0x33 0xFF 0xFF 0xFF |
| Returned when using get command for a string. Each byte is converted to char. |
| **data**: ab123 |
| 26 | 0x71 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 8 | Numeric Data Enclosed | 0x71 0x01 0x02 0x03 0x04 0xFF 0xFF 0xFF |
| Returned when get command to return a number 4 byte 32-bit value in little endian order. |
| (0x01+0x02\*256+0x03\*65536+0x04\*16777216) |
| **data**: 67305985 |
| 27 | 0x86 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 4 | Auto Entered Sleep Mode | 0x86 0xFF 0xFF 0xFF |
| Returned when Nextion enters sleep automatically Using sleep=1 will not return an 0x86 |
| 28 | 0x87 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 4 | Auto Wake from Sleep | 0x87 0xFF 0xFF 0xFF |
| Returned when Nextion leaves sleep automatically Using sleep=0 will not return an 0x87 |
| 29 | 0x88 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 4 | Nextion Ready | 0x88 0xFF 0xFF 0xFF |
| Returned when Nextion has powered up and is now initialized successfully |
| 30 | 0x89 https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 4 | Start microSD Upgrade | 0x89 0xFF 0xFF 0xFF |
| Returned when power on detects inserted microSD and begins Upgrade by microSD process |
| 31 | 0xFD https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 4 | Transparent Data Finished | 0xFD 0xFF 0xFF 0xFF |
| Returned when all requested bytes of Transparent Data mode have been received, and is now leaving transparent data mode (see [1.16](https://nextion.tech/resource/documents/instruction-set/#s1_16)) |
| 32 | 0xFE https://cdn.nextion.tech/wp-content/uploads/2019/07/sA.png | 4 | Transparent Data Ready | 0xFE 0xFF 0xFF 0xFF |
| Returned when requesting Transparent Data mode, and device is now ready to begin receiving the specified quantity of data (see [1.16](https://nextion.tech/resource/documents/instruction-set/#s1_16)) |